**Safety Review Preparation**

| **Seismic Data Presentation Question** | **Answer** |
| --- | --- |
| (1) Is the seabed signature clearly visible and can the polarity be established? | {{srr\_checklist.q1}} |
| (2) Have the seismic data been displayed with and without an interpretation? | {{srr\_checklist.q2}} |
| (3) Have both a time and a depth section been presented? | {{srr\_checklist.q3}} |
| (4) Do the final site displays result in the drill stick representing about half of the vertical section? (This is not required for regional displays.) | {{srr\_checklist.q4}} |
| (5) Has the depth of proposed penetration been marked? (This should include the target depth and the total depth of penetration if a logging tool is to be used. The marking “stick” should also include an estimate of uncertainty.) | {{srr\_checklist.q5}} |
| (6) Have key geologic and/or safety issues been highlighted on the seismic data? | {{srr\_checklist.q6}} |
| (7) Have seismic attributes been presented in color rather than black and white? | {{srr\_checklist.q7}} |
| (8) Are the vertical and horizontal scales on associated strike- and dip-sections the same? | {{srr\_checklist.q8}} |
| (9) Have intersections with cross-lines been clearly labeled? | {{srr\_checklist.q9}} |
| (10) Have CDP or shot points been appropriately labeled? | {{srr\_checklist.q10}} |
| (11) Are both vertical and horizontal scales present (preferably on the axis)? | {{srr\_checklist.q11}} |
| (12) Has a summary of acquisition and processing been provided? | {{srr\_checklist.q12}} |
| (13) Is the processing appropriate for imaging the target depth? | {{srr\_checklist.q13}} |
| (14) Has the information utilized to establish the time-depth conversion been provided? | {{srr\_checklist.q14}} |

| **Seismic Data Presentation Question** | **Answer** |
| --- | --- |
| (15) On the map, has directionality been established with an arrow or a latitude/longitude grid? | {{srr\_checklist.q15}} |
| (16) Has a suitable map scale been provided? | {{srr\_checklist.q16}} |
| (17) Are contours appropriately labeled with units identified? | {{srr\_checklist.q17}} |
| (18) Are all necessary seismic track lines identified on maps, with shot points labeled at a regular interval? | {{srr\_checklist.q18}} |
| (19) Has the resolution of the grid been provided? And, has the appropriate scale bar been presented? | {{srr\_checklist.q19}} |
| (20) Do all maps share a common coordinate reference system? | {{srr\_checklist.q20}} |

| **Comments** |
| --- |
| {{srr\_checklist.comments}} |